MyHealth@Eu Patient Summary
1.0.0-poc - qa-preview 150

MyHealth@Eu Patient Summary - Downloaded Version 1.0.0-poc See the Directory of published versions

## Resource Profile: Device: MyHealth@EU EPS

Official URL: http://fhir.ehdsi.eu/eps/StructureDefinition/device-eps-myhealtheu | Version: 1.0.0-poc
Standards status: Draft | Maturity Level: 1 | Computable Name: DeviceMyHealthEuEps
Copyright/Legal: Copyright European Union, represented by the European Commission - DG SANTE. Licenced under CC-BY-4.0.

This profile constrains the Device resource for the purpose of the MyHealth@EU EPS.

Usages:

- Use this Profile: Bundle: MyHealth@EU EPS
- Refer to this Profile: DeviceUseStatement: MyHealth@EU EPS
- Examples for this Profile: Device/0b89dcab-1d0c-44fa-a958-3131452d8cca

You can also check for usages in the FHIR IG Statistics

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Key Elements Table
- Differential Table
- Snapshot Table
- Statistics/References
- All

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | DeviceEuEps | Item used in healthcare This profile also imposes the profile Device (IPS) (2.0.0)
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | O | 0..* | Identifier | Device Identifier
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
type | O | 0..1 | CodeableConcept | Type of device. Preferably valued by using SNOMED CT. The absence of information, or of devices relevant for purpose of this IPS, shall be explicitly stated by using the codes included in the absent-or-unknown-devices-uv-ips value set. Binding: eHDSI Medical Device With Exceptions (required)
Additional Bindings | Purpose
eHDSI Medical Device | candidate
Obligations | Actor | Source
SHALL:populate-if-known | Creator (IPS) | from Device (EPS)
SHALL:handle | Consumer (IPS) | from Device (EPS)
SHOULD:display | Consumer (IPS) | from Device (EPS)
patient |  | 1..1 | Reference(Patient: MyHealth@EU EPS) | Patient to whom Device is affixed
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
Device.status | Base | required | FHIRDeviceStatus | 📍4.0.1 | FHIR Std.
Device.type | Base | required | eHDSI Medical Device With Exceptions | 📦1.0.0 | MyHealth@EU Core v1.0

#### Constraints

Id | Grade | Path(s) | Description | Expression
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

This structure is derived from DeviceEuEps

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  |  | DeviceEuEps | This profile also imposes the profile Device (IPS) (2.0.0)
identifier | O | 0..* | Identifier | Device Identifier
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
deviceName |  |  |  |
name | O | 1..1 | string | Device Name
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
type |  | 0..1 | CodeableConcept | Type of device. Preferably valued by using SNOMED CT. The absence of information, or of devices relevant for purpose of this IPS, shall be explicitly stated by using the codes included in the absent-or-unknown-devices-uv-ips value set. Binding: eHDSI Medical Device With Exceptions (required)
patient |  | 1..1 | Reference(Patient: MyHealth@EU EPS) | Patient to whom Device is affixed
Documentation for this format

#### Terminology Bindings (Differential)

Path | Status | Usage | ValueSet | Version | Source
Device.type | Base | required | eHDSI Medical Device With Exceptions | 📦1.0.0 | MyHealth@EU Core v1.0

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | DeviceEuEps | Item used in healthcare This profile also imposes the profile Device (IPS) (2.0.0)
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | O | 0..* | Identifier | Device Identifier
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Device Manufacturer
manufactureDate |  | 0..1 | dateTime | Device Manufacture Date
expirationDate |  | 0..1 | dateTime | Device Expiration Date
lotNumber |  | 0..1 | string | Device Lot Number
serialNumber |  | 0..1 | string | Device Serial Number
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name | O | 1..1 | string | Device Name
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | Device Model Number
partNumber |  | 0..1 | string | The part number of the device
type | O | 0..1 | CodeableConcept | Type of device. Preferably valued by using SNOMED CT. The absence of information, or of devices relevant for purpose of this IPS, shall be explicitly stated by using the codes included in the absent-or-unknown-devices-uv-ips value set. Binding: eHDSI Medical Device With Exceptions (required)
Additional Bindings | Purpose
eHDSI Medical Device | candidate
Obligations | Actor | Source
SHALL:populate-if-known | Creator (IPS) | from Device (EPS)
SHALL:handle | Consumer (IPS) | from Device (EPS)
SHOULD:display | Consumer (IPS) | from Device (EPS)
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | Device Version
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 1..1 | Reference(Patient: MyHealth@EU EPS) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device Note
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
Device.language | Base | preferred | Common Languages | 📍4.0.1 | FHIR Std.
Device.udiCarrier.entryType | Base | required | UDIEntryType | 📍4.0.1 | FHIR Std.
Device.status | Base | required | FHIRDeviceStatus | 📍4.0.1 | FHIR Std.
Device.statusReason | Base | extensible | FHIRDeviceStatusReason | 📍4.0.1 | FHIR Std.
Device.deviceName.type | Base | required | DeviceNameType | 📍4.0.1 | FHIR Std.
Device.type | Base | required | eHDSI Medical Device With Exceptions | 📦1.0.0 | MyHealth@EU Core v1.0

#### Constraints

Id | Grade | Path(s) | Description | Expression
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

This structure is derived from DeviceEuEps

Summary

Mandatory: 1 element

Structures

This structure refers to these other structures:

- Patient: MyHealth@EU EPS (http://fhir.ehdsi.eu/eps/StructureDefinition/patient-myhealtheu-eps)

Maturity: 1

Key Elements View

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | DeviceEuEps | Item used in healthcare This profile also imposes the profile Device (IPS) (2.0.0)
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | O | 0..* | Identifier | Device Identifier
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
type | O | 0..1 | CodeableConcept | Type of device. Preferably valued by using SNOMED CT. The absence of information, or of devices relevant for purpose of this IPS, shall be explicitly stated by using the codes included in the absent-or-unknown-devices-uv-ips value set. Binding: eHDSI Medical Device With Exceptions (required)
Additional Bindings | Purpose
eHDSI Medical Device | candidate
Obligations | Actor | Source
SHALL:populate-if-known | Creator (IPS) | from Device (EPS)
SHALL:handle | Consumer (IPS) | from Device (EPS)
SHOULD:display | Consumer (IPS) | from Device (EPS)
patient |  | 1..1 | Reference(Patient: MyHealth@EU EPS) | Patient to whom Device is affixed
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
Device.status | Base | required | FHIRDeviceStatus | 📍4.0.1 | FHIR Std.
Device.type | Base | required | eHDSI Medical Device With Exceptions | 📦1.0.0 | MyHealth@EU Core v1.0

#### Constraints

Id | Grade | Path(s) | Description | Expression
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

Differential View

This structure is derived from DeviceEuEps

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  |  | DeviceEuEps | This profile also imposes the profile Device (IPS) (2.0.0)
identifier | O | 0..* | Identifier | Device Identifier
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
deviceName |  |  |  |
name | O | 1..1 | string | Device Name
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
type |  | 0..1 | CodeableConcept | Type of device. Preferably valued by using SNOMED CT. The absence of information, or of devices relevant for purpose of this IPS, shall be explicitly stated by using the codes included in the absent-or-unknown-devices-uv-ips value set. Binding: eHDSI Medical Device With Exceptions (required)
patient |  | 1..1 | Reference(Patient: MyHealth@EU EPS) | Patient to whom Device is affixed
Documentation for this format

#### Terminology Bindings (Differential)

Path | Status | Usage | ValueSet | Version | Source
Device.type | Base | required | eHDSI Medical Device With Exceptions | 📦1.0.0 | MyHealth@EU Core v1.0

Snapshot View

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* | DeviceEuEps | Item used in healthcare This profile also imposes the profile Device (IPS) (2.0.0)
id | Σ | 0..1 | id | Logical id of this artifact
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | O | 0..* | Identifier | Device Identifier
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Device Manufacturer
manufactureDate |  | 0..1 | dateTime | Device Manufacture Date
expirationDate |  | 0..1 | dateTime | Device Expiration Date
lotNumber |  | 0..1 | string | Device Lot Number
serialNumber |  | 0..1 | string | Device Serial Number
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name | O | 1..1 | string | Device Name
Obligations | Actor
SHOULD:handle | MyHealth@EU Handler
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | Device Model Number
partNumber |  | 0..1 | string | The part number of the device
type | O | 0..1 | CodeableConcept | Type of device. Preferably valued by using SNOMED CT. The absence of information, or of devices relevant for purpose of this IPS, shall be explicitly stated by using the codes included in the absent-or-unknown-devices-uv-ips value set. Binding: eHDSI Medical Device With Exceptions (required)
Additional Bindings | Purpose
eHDSI Medical Device | candidate
Obligations | Actor | Source
SHALL:populate-if-known | Creator (IPS) | from Device (EPS)
SHALL:handle | Consumer (IPS) | from Device (EPS)
SHOULD:display | Consumer (IPS) | from Device (EPS)
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | Device Version
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient |  | 1..1 | Reference(Patient: MyHealth@EU EPS) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device Note
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format

#### Terminology Bindings

Path | Status | Usage | ValueSet | Version | Source
Device.language | Base | preferred | Common Languages | 📍4.0.1 | FHIR Std.
Device.udiCarrier.entryType | Base | required | UDIEntryType | 📍4.0.1 | FHIR Std.
Device.status | Base | required | FHIRDeviceStatus | 📍4.0.1 | FHIR Std.
Device.statusReason | Base | extensible | FHIRDeviceStatusReason | 📍4.0.1 | FHIR Std.
Device.deviceName.type | Base | required | DeviceNameType | 📍4.0.1 | FHIR Std.
Device.type | Base | required | eHDSI Medical Device With Exceptions | 📦1.0.0 | MyHealth@EU Core v1.0

#### Constraints

Id | Grade | Path(s) | Description | Expression
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources | `contained.contained.empty()`
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource | `contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty()`
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated | `contained.meta.versionId.empty() and contained.meta.lastUpdated.empty()`
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label | `contained.meta.security.empty()`
dom-6 | best practice | Device | A resource should have narrative for robust management | `text.`div`.exists()`
ele-1 | error | **ALL** elements | All FHIR elements must have a @value or children | `hasValue() or (children().count() > id.count())`
ext-1 | error | **ALL** extensions | Must have either extensions or value[x], not both | `extension.exists() != value.exists()`

This structure is derived from DeviceEuEps

Summary

Mandatory: 1 element

Structures

This structure refers to these other structures:

- Patient: MyHealth@EU EPS (http://fhir.ehdsi.eu/eps/StructureDefinition/patient-myhealtheu-eps)

Maturity: 1

Other representations of profile: CSV, Excel, Schematron